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	FROM:
	Tournament Director  – David Garland
	

	EVENT:
	The 2010 Ryder Cup - Twenty Ten Course

	

	GREENS
	

	
Type of grass
	- Creeping bent/poa

	       Height of cut
	- 3.00mm

	
Speed/stimpmeter reading
	- 10’6’’ 

	
	

	FAIRWAYS
	

	
Type of grass
	- Rye, bent, fescue, poa

	
Height of cut
	- 11mm

	
General width and contouring
	- 

	
	

	TEES / COLLARS
	

	
Type of grass
	- Rye, bent, fescue, poa

	
Height of cut
	- 9 mm

	
	

	ROUGH
	

	
Type of grass
	- Fescue, smooth stalked meadow 

	
Height of cut - semi


- intermediate

- rough
	- 32mm
- 64mm
- 100 – 120mm

	
	

	WEATHER
	

	
Weather in advance
	- Generally dry with occasional showers

	
Forecast for tournament
	- Mild and breezy with scattered showers

	COURSE
	

	      Opened                                     
	- 2007 (original Wentwood Hills course opened in 1999)

	      Course designer
	- Holes 1-5, 14 and 16-18 are completely new (designed by Ross McMurray from European Golf Design). The remaining holes, which formed part of the Wentwood Hills course, were originally designed by Robert Trent Jones Jnr, with some minor modification by EGD.

	
Undulating / flat
	- Generally quite flat with change of elevation on holes 15-18.

	
Tree lined / exposed
	- Open to the elements

	
Many / few water hazards
	- There are water hazards on 10 of the holes

	OTHER FEATURES
	

	Any other features of the course or the event that may be of interest to web readers
	- The course sits in the USK Valley and borders to the river USK.


